Magic 271485
Revision Verdi_O-2018.09-SP2

; Window Layout <x> <y> <width> <height> <signalwidth> <valuewidth>
viewPort 0 27 1920 392 256 65

; File list:
; openDirFile [-d delimiter] [-s time_offset] [-rf auto_bus_rule_file] path_name file_name
openDirFile -d / "" "/home/shbyang/Desktop/workplace/lin-win-share/DA4008_V1.2/sim/chip_top/work_RTL/sine_1g/verdplus_000.fsdb"

; file time scale:
; fileTimeScale ### s|ms|us|ns|ps

; signal spacing:
signalSpacing 5

; windowTimeUnit is used for zoom, cursor & marker
; waveform viewport range
zoom 0.000000 25862591.942020
cursor 7001856.000000
marker 479076480.000000

; user define markers
; userMarker time_pos marker_name color linestyle
; visible top row signal index
top 15
; marker line index
markerPos 40

; event list
; addEvent event_name event_expression
; curEvent event_name



COMPLEX_EVENT_BEGIN


COMPLEX_EVENT_END



; toolbar current search type
; curSTATUS search_type
curSTATUS ByChange


addGroup "SPI" -e FALSE
activeDirFile "" "/home/shbyang/Desktop/workplace/lin-win-share/DA4008_V1.2/sim/chip_top/work_RTL/sine_1g/verdplus_000.fsdb"
addSignal -h 15 /TB/U_da4008_chip_top/PI_sclk
addSignal -h 15 -holdScope PI_csn
addSignal -h 15 -holdScope PI_mosi
addSignal -h 15 -holdScope PO_miso
addGroup "SYS" -e FALSE
addSignal -h 15 /TB/U_da4008_chip_top/clk
addSignal -h 15 -holdScope PI_async_rstn
addSignal -h 15 -holdScope PI_sync_in
addSignal -h 15 -holdScope PO_sync_out
addSignal -h 15 -holdScope PO_irq
addGroup "LVDS" -e FALSE
addSignal -h 15 /TB/U_da4008_chip_top/lvds_clk[0:0]
addSignal -h 15 -holdScope lvds_data[3:0]
addSignal -h 15 -holdScope lvds_valid[0:0]
addGroup "DAC" -e FALSE
addSignal -h 15 /TB/start
addSignal -w analog -ds pwc -h 98 -holdScope cs_wave[7:0]
addSignal -h 15 /TB/U_da4008_chip_top/MSB_OUT[63:0]
addSignal -h 15 -holdScope LSB_OUT[63:0]
addSignal -h 15 -holdScope MSB_DUM[63:0]
addSignal -h 15 -holdScope DEM_VLD
addGroup "A_sram"
addSignal -h 15 /TB/U_da4008_chip_top/digital_top/wave_awrdata[511:0]
addSignal -h 15 -holdScope wave_awren[0:0]
addSignal -h 15 -holdScope wave_arwaddr[12:0]
addSignal -h 15 -holdScope wave_awrmask[63:0]
addGroup "B_sram" -e FALSE
addSignal -h 15 /TB/U_da4008_chip_top/digital_top/slv[2]/din[31:0]
addSignal -h 15 -holdScope wren
addSignal -h 15 -holdScope addr[18:0]
addSignal -h 15 -holdScope rden
addSignal -h 15 -holdScope dout[31:0]
addGroup "G7"
addSignal -expanded -h 15 /TB/U_da4008_chip_top/digital_top/dut/serial_in[3:0]
addSignal -h 15 -holdScope serial_in[3]
addSignal -h 15 -holdScope serial_in[2]
addSignal -h 15 -holdScope serial_in[1]
addSignal -h 15 -holdScope serial_in[0]
addSignal -h 15 -holdScope train_ready
addSignal -h 15 -holdScope frame_done
addGroup "G8"

; getSignalForm Scope Hierarchy Status
; active file of getSignalForm

