: // Synopsys, Inc.
: //

: // Generated by: VCS Coverage Metrics O-2018.09-SP2_Full64
: // User: shbyang
: // Date: Fri Mar 13 16:24:00 2026

: Disabling fsm sequence coverage for module \$unit::../../lib/tphn28hpcpgv18.v::../../lib/tsdn28hpcpuhdb4096x128m4mw_170a_ffg0p99v0c.v...@348857874  ... 
: Disabling fsm sequence coverage for module PCLAMP_G ... 
: Disabling fsm sequence coverage for module PCLAMPC_H_G ... 
: Disabling fsm sequence coverage for module PCLAMPC_V_G ... 
: Disabling fsm sequence coverage for module PDB3A_H_G ... 
: Disabling fsm sequence coverage for module PDB3A_V_G ... 
: Disabling fsm sequence coverage for module PDB3AC_H_G ... 
: Disabling fsm sequence coverage for module PDB3AC_V_G ... 
: Disabling fsm sequence coverage for module PDDW04DGZ_H_G ... 
: Disabling fsm sequence coverage for module PDDW04DGZ_V_G ... 
: Disabling fsm sequence coverage for module PDDW04SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PDDW08DGZ_H_G ... 
: Disabling fsm sequence coverage for module PDDW08DGZ_V_G ... 
: Disabling fsm sequence coverage for module PDDW08SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PDDW08SDGZ_V_G ... 
: Disabling fsm sequence coverage for module PDDW12DGZ_H_G ... 
: Disabling fsm sequence coverage for module PDDW12DGZ_V_G ... 
: Disabling fsm sequence coverage for module PDDW12SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PDDW12SDGZ_V_G ... 
: Disabling fsm sequence coverage for module PDDW16DGZ_H_G ... 
: Disabling fsm sequence coverage for module PDDW16DGZ_V_G ... 
: Disabling fsm sequence coverage for module PDDW16SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PDDW16SDGZ_V_G ... 
: Disabling fsm sequence coverage for module PDUW04DGZ_H_G ... 
: Disabling fsm sequence coverage for module PDUW04DGZ_V_G ... 
: Disabling fsm sequence coverage for module PDUW04SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PDUW08DGZ_H_G ... 
: Disabling fsm sequence coverage for module PDUW08DGZ_V_G ... 
: Disabling fsm sequence coverage for module PDUW08SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PDUW12DGZ_H_G ... 
: Disabling fsm sequence coverage for module PDUW12DGZ_V_G ... 
: Disabling fsm sequence coverage for module PDUW12SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PDUW12SDGZ_V_G ... 
: Disabling fsm sequence coverage for module PDUW16DGZ_H_G ... 
: Disabling fsm sequence coverage for module PDUW16DGZ_V_G ... 
: Disabling fsm sequence coverage for module PDUW16SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PDUW16SDGZ_V_G ... 
: Disabling fsm sequence coverage for module PDXOEDG_H_G ... 
: Disabling fsm sequence coverage for module PDXOEDG_V_G ... 
: Disabling fsm sequence coverage for module PENDCAP_G ... 
: Disabling fsm sequence coverage for module PENDCAPA_G ... 
: Disabling fsm sequence coverage for module PRCUT_G ... 
: Disabling fsm sequence coverage for module PRCUTA_G ... 
: Disabling fsm sequence coverage for module PRDW08DGZ_H_G ... 
: Disabling fsm sequence coverage for module PRDW08DGZ_V_G ... 
: Disabling fsm sequence coverage for module PRDW08SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PRDW08SDGZ_V_G ... 
: Disabling fsm sequence coverage for module PRDW12DGZ_H_G ... 
: Disabling fsm sequence coverage for module PRDW12DGZ_V_G ... 
: Disabling fsm sequence coverage for module PRDW12SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PRDW12SDGZ_V_G ... 
: Disabling fsm sequence coverage for module PRDW16DGZ_H_G ... 
: Disabling fsm sequence coverage for module PRDW16DGZ_V_G ... 
: Disabling fsm sequence coverage for module PRDW16SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PRDW16SDGZ_V_G ... 
: Disabling fsm sequence coverage for module PRUW08DGZ_H_G ... 
: Disabling fsm sequence coverage for module PRUW08DGZ_V_G ... 
: Disabling fsm sequence coverage for module PRUW08SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PRUW08SDGZ_V_G ... 
: Disabling fsm sequence coverage for module PRUW12DGZ_H_G ... 
: Disabling fsm sequence coverage for module PRUW12DGZ_V_G ... 
: Disabling fsm sequence coverage for module PRUW12SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PRUW12SDGZ_V_G ... 
: Disabling fsm sequence coverage for module PRUW16DGZ_H_G ... 
: Disabling fsm sequence coverage for module PRUW16DGZ_V_G ... 
: Disabling fsm sequence coverage for module PRUW16SDGZ_H_G ... 
: Disabling fsm sequence coverage for module PRUW16SDGZ_V_G ... 
: Disabling fsm sequence coverage for module PVDD1A_H_G ... 
: Disabling fsm sequence coverage for module PVDD1A_V_G ... 
: Disabling fsm sequence coverage for module PVDD1AC_H_G ... 
: Disabling fsm sequence coverage for module PVDD1AC_V_G ... 
: Disabling fsm sequence coverage for module PVDD1ANA_H_G ... 
: Disabling fsm sequence coverage for module PVDD1ANA_V_G ... 
: Disabling fsm sequence coverage for module PVDD1DGZ_H_G ... 
: Disabling fsm sequence coverage for module PVDD1DGZ_V_G ... 
: Disabling fsm sequence coverage for module PVDD2ANA_H_G ... 
: Disabling fsm sequence coverage for module PVDD2ANA_V_G ... 
: Disabling fsm sequence coverage for module PVDD2DGZ_H_G ... 
: Disabling fsm sequence coverage for module PVDD2DGZ_V_G ... 
: Disabling fsm sequence coverage for module PVDD2POC_H_G ... 
: Disabling fsm sequence coverage for module PVDD2POC_V_G ... 
: Disabling fsm sequence coverage for module PVDD3A_H_G ... 
: Disabling fsm sequence coverage for module PVDD3A_V_G ... 
: Disabling fsm sequence coverage for module PVDD3AC_H_G ... 
: Disabling fsm sequence coverage for module PVDD3AC_V_G ... 
: Disabling fsm sequence coverage for module PVSS1A_H_G ... 
: Disabling fsm sequence coverage for module PVSS1A_V_G ... 
: Disabling fsm sequence coverage for module PVSS1AC_H_G ... 
: Disabling fsm sequence coverage for module PVSS1AC_V_G ... 
: Disabling fsm sequence coverage for module PVSS1ANA_H_G ... 
: Disabling fsm sequence coverage for module PVSS1ANA_V_G ... 
: Disabling fsm sequence coverage for module PVSS1DGZ_H_G ... 
: Disabling fsm sequence coverage for module PVSS1DGZ_V_G ... 
: Disabling fsm sequence coverage for module PVSS2A_H_G ... 
: Disabling fsm sequence coverage for module PVSS2A_V_G ... 
: Disabling fsm sequence coverage for module PVSS2AC_H_G ... 
: Disabling fsm sequence coverage for module PVSS2AC_V_G ... 
: Disabling fsm sequence coverage for module PVSS2ANA_H_G ... 
: Disabling fsm sequence coverage for module PVSS2ANA_V_G ... 
: Disabling fsm sequence coverage for module PVSS2DGZ_H_G ... 
: Disabling fsm sequence coverage for module PVSS2DGZ_V_G ... 
: Disabling fsm sequence coverage for module PVSS3A_H_G ... 
: Disabling fsm sequence coverage for module PVSS3A_V_G ... 
: Disabling fsm sequence coverage for module PVSS3AC_H_G ... 
: Disabling fsm sequence coverage for module PVSS3AC_V_G ... 
: Disabling fsm sequence coverage for module PVSS3DGZ_H_G ... 
: Disabling fsm sequence coverage for module PVSS3DGZ_V_G ... 
: Disabling fsm sequence coverage for module sirv_gnrl_xchecker ... 
: Disabling fsm sequence coverage for module sirv_gnrl_dffl ... 
: Disabling fsm sequence coverage for module sirv_gnrl_ltch ... 
: Disabling fsm sequence coverage for module clk_gen ... 
: Disabling fsm sequence coverage for module reset_tb ... 
: Disabling fsm sequence coverage for module TB ... 
: Disabling fsm sequence coverage for module TB.clk_inst ... 
: Disabling fsm sequence coverage for module TB.clk_40g_inst ... 
: Disabling fsm sequence coverage for module TB.spi_bus ... 
: Disabling fsm sequence coverage for module TB.lvds_bus ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_iopad ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_iopad.PDUW08SDGZ_V_G_async_rstn ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_iopad.PDDW04SDGZ_V_G_sync_in ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_iopad.PDDW08SDGZ_V_G_sync_out ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_iopad.PDUW04SDGZ_V_G_sclk ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_iopad.PDUW04SDGZ_V_G_csn ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_iopad.PDUW08SDGZ_V_G_mosi ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_iopad.PDUW08SDGZ_V_G_miso ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_iopad.PDUW08SDGZ_V_G_irq ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.mst ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.bit_cnt_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.bit_cnt_r_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.cmd_or_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.second_falling_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.wnr_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.addr_m5b_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.addr_l8b_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.chipid_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.rddata_update_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.addr_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.oen_dffrs ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.miso_reg_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[0].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[1].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[2].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[3].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[4].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[5].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[6].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[7].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[8].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[9].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[10].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[11].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[12].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[13].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[14].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[15].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[16].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[17].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[18].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[19].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[20].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[21].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[22].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[23].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[24].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[25].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[26].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[27].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[28].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[29].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[30].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[31].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.sclk_reg_dffrs ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.csn_reg_dffrs ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.mosi_reg_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.cnt_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.initaddr_vld_r_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.initaddr_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.cmd_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.chipid_vld_r_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.chipid_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.state_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.second_falling_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.addr_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.wrdata_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.wren_r_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.wren_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.rden_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.rddata_reg_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_dout_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.oen_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[0].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[1].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[2].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[3].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[4].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[5].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[6].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[7].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[8].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[9].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[10].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[11].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[12].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[13].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[14].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[15].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[16].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[17].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[18].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[19].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[20].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[21].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[22].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[23].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[24].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[25].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[26].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[27].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[28].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[29].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[30].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[31].spi_din_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[0].CMD_REG.rwaddr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[0].CMD_REG.wrdata_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[0].CMD_REG.wren_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[0].CMD_REG.reen_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[1].CMD_REG.rwaddr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[1].CMD_REG.wrdata_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[1].CMD_REG.wren_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[1].CMD_REG.reen_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[2].CMD_REG.rwaddr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[2].CMD_REG.wrdata_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[2].CMD_REG.wren_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[2].CMD_REG.reen_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[3].CMD_REG.rwaddr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[3].CMD_REG.wrdata_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[3].CMD_REG.wren_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[3].CMD_REG.reen_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.testr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.sfrtr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.syncr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.syncr16_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.syncr16_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.sync_oen_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.rampctr_dfflrs ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.ramp_ifs_dfflrs ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.doselr_dfflrs ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdsftr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdstfr_dfflrs ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdstsr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdsthr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdstamr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdsdser_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdstaor_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.llvdssr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdsfcsr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdscecr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdsfstr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdststr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.imr_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.cnt_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.sys_soft_rstn_r_dffls ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.rddata_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.train_ready_r_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.crc_error_r_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.cphase_adj_req_r_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.link_down_r_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.cmd_fifo_full_r_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.cmd_fifo_empty_r_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.isr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.misr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.irq_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_rst_gen_unit ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_rst_gen_unit.ch0_rstn_sync ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_rst_gen_unit.ch1_rstn_sync ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_rst_gen_unit.ch2_rstn_sync ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_rst_gen_unit.ch3_rstn_sync ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_SRC_INIT ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_SRC_INIT.SIM ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_SYNC_CLR_S ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_DEST_INIT ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_DEST_INIT.SIM ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_FB_DEST ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_FB_DEST.SIM ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_ACK ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_ACK.SIM ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_SYNC ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.U_prefill ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.U_prefill.delay_counter_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.U_prefill.prefill_start_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.U_prefill.prefilling_r_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.U_prefill.prefill_done_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.lane0_reg_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.lane1_reg_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.lane2_reg_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.lane3_reg_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.bit_counter_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.match_counter_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.state_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.delay_tap_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.tap_adj_req_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.link_down_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.train_ready_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.data_buf_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.match_head_start_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.data_counter_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.valid_int_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.descram_valid_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.data_in_reg_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.train_status_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_descrambler ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_descrambler.u0 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_descrambler.u1 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_descrambler.u2 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_descrambler.u3 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.u_fifo ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.u_fifo.spram ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.u_fifo.spram.bhv_spram ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.word_state_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.current_fifo_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.current_word_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.word_valid_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.data_len_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.data_cnt_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.state_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.cur_block_offset_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.block_done_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.base_addr_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.cur_block_addr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.cur_block_addr_r_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.wr_addr_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.wr_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.byte_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.wr_en_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.frame_done_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.u_crc32 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.crc_clear_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.crc_error_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.frame_status_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[0].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[1].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[2].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[3].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[4].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[5].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[6].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[7].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[8].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[9].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[10].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[11].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[12].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[13].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[14].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[15].cur_block_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[0].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[1].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[2].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[3].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[4].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[5].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[6].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[7].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[8].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[9].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[10].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[11].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[12].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[13].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[14].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[15].cur_block_mask_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.sync_in_syncer ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.sync_in_syncer.data_temp0_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.sync_in_syncer.SYNCER[1].data_tempn0_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.sync_out_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.pulse_inst_sync ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.start_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.sync_start_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.state_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.cycle_num_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.base_addr_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.wave_leng_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.hold_leng_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.addr_cnt_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.wave_cnt_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.hold_cnt_c_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.sram_rd_en_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.sram_rd_addr_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.last_sram_rd_en_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.last_wave_data_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.last_rddata_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.wave_vld_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.hold_vld_n_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.hold_vld_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.wave_valid_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.wave_data_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.cmd_fifo_inst ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.cmd_fifo_inst.spram ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.cmd_fifo_inst.spram.bhv_spram ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_sram_muxin ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_sram_muxout ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.U_sram_dmux_w ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U0_tsdn28hpcpuhdb4096x128m4mw_170a ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U0_tsdn28hpcpuhdb4096x128m4mw_170a.MX ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U1_tsdn28hpcpuhdb4096x128m4mw_170a ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U1_tsdn28hpcpuhdb4096x128m4mw_170a.MX ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U2_tsdn28hpcpuhdb4096x128m4mw_170a ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U2_tsdn28hpcpuhdb4096x128m4mw_170a.MX ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U3_tsdn28hpcpuhdb4096x128m4mw_170a ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U3_tsdn28hpcpuhdb4096x128m4mw_170a.MX ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U0_tsdn28hpcpuhdb4096x128m4mw_170a ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U0_tsdn28hpcpuhdb4096x128m4mw_170a.MX ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U1_tsdn28hpcpuhdb4096x128m4mw_170a ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U1_tsdn28hpcpuhdb4096x128m4mw_170a.MX ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U2_tsdn28hpcpuhdb4096x128m4mw_170a ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U2_tsdn28hpcpuhdb4096x128m4mw_170a.MX ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U3_tsdn28hpcpuhdb4096x128m4mw_170a ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U3_tsdn28hpcpuhdb4096x128m4mw_170a.MX ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_ramp_gen ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.dacif_vld_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[0].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[1].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[2].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[3].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[4].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[5].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[6].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[7].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[8].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[9].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[10].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[11].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[12].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[13].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[14].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[15].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[16].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[17].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[18].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[19].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[20].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[21].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[22].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[23].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[24].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[25].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[26].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[27].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[28].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[29].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[30].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[31].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[32].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[33].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[34].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[35].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[36].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[37].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[38].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[39].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[40].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[41].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[42].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[43].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[44].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[45].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[46].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[47].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[48].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[49].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[50].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[51].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[52].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[53].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[54].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[55].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[56].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[57].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[58].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[59].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[60].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[61].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[62].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[63].mux_dfflr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[0].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[1].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[2].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[3].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[4].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[5].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[6].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[7].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[8].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[9].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[10].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[11].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[12].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[13].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[14].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[15].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[16].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[17].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[18].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[19].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[20].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[21].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[22].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[23].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[24].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[25].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[26].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[27].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[28].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[29].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[30].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[31].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[32].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[33].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[34].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[35].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[36].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[37].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[38].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[39].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[40].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[41].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[42].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[43].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[44].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[45].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[46].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[47].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[48].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[49].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[50].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[51].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[52].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[53].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[54].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[55].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[56].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[57].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[58].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[59].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[60].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[61].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[62].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[63].dout_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.rtermr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.prbsr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set0r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set1r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set2r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set3r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set4r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set5r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set6r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set7r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set8r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set9r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set10r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set11r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set12r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set13r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set14r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set15r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set16r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set17r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set18r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set19r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set20r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set21r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set22r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set23r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set24r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set25r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set26r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set27r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set28r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set29r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set30r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set31r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.casaddrr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.casdwr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.imctr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.ibleedctr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.iclkcmlr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.currsvr0_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.currsvr1_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.rddata_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalrstnr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.cclkdccenr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.casclkctr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccaldccqecpir_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalqecctr1_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.biasct3r_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalpictr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalcrossctr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalrsvr0_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalrsvr1_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.selck10gdr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.selck2p5gdr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.selck625mdr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.p2sdataenr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.enallpr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.enpipr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.clkdivrstnr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.p2srsvr0_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.p2srsvr1_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ckrxswr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.rstckr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ctrzinr_dfflrd ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.rddata_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.slv[0] ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.slv[1] ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.slv[2] ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.digital_top.slv[3] ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.DEM_VLD_dffr ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_0 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_1 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_2 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_3 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_4 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_5 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_6 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_7 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_8 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_9 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_10 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_11 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_12 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_13 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_14 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_15 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_16 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_17 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_18 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_19 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_20 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_21 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_22 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_23 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_24 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_25 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_26 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_27 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_28 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_29 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_30 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_31 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_32 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_33 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_34 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_35 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_36 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_37 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_38 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_39 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_40 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_41 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_42 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_43 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_44 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_45 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_46 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_47 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_48 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_49 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_50 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_51 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_52 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_53 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_54 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_55 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_56 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_57 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_58 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_59 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_60 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_61 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_62 ... 
: Disabling fsm sequence coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_63 ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[0].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[1].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[2].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[3].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[4].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[5].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[6].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[7].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[8].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[9].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[10].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[11].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[12].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[13].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[14].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[15].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[16].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[17].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[18].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[19].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[20].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[21].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[22].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[23].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[24].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[25].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[26].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[27].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[28].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[29].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[30].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk1[31].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[32].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[33].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[34].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[35].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[36].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[37].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[38].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[39].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[40].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[41].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[42].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[43].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[44].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[45].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[46].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[47].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[48].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[49].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[50].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[51].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[52].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[53].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[54].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[55].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[56].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[57].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[58].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[59].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[60].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[61].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[62].U_DEM_Reverse ... 
: Disabling fsm sequence coverage for module TB.U_DEM_Reverse_64CH.genblk2[63].U_DEM_Reverse ... 
: Starting toggle coverage for module sirv_gnrl_xchecker
: Starting toggle coverage for module sirv_gnrl_dffl
: Starting toggle coverage for module sirv_gnrl_ltch
: Starting toggle coverage for module clk_gen
: Starting toggle coverage for module reset_tb
: Starting toggle coverage for module TB
: Starting toggle coverage for module TB.clk_inst
: Starting toggle coverage for module TB.clk_40g_inst
: Starting toggle coverage for module TB.spi_bus
: Starting toggle coverage for module TB.lvds_bus
: Starting toggle coverage for module TB.U_da4008_chip_top
: Starting toggle coverage for module TB.U_da4008_chip_top.U_iopad
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.mst
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.bit_cnt_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.bit_cnt_r_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.cmd_or_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.second_falling_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.wnr_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.addr_m5b_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.addr_l8b_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.chipid_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.rddata_update_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.addr_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.oen_dffrs
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.miso_reg_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[0].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[1].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[2].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[3].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[4].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[5].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[6].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[7].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[8].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[9].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[10].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[11].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[12].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[13].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[14].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[15].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[16].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[17].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[18].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[19].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[20].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[21].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[22].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[23].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[24].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[25].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[26].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[27].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[28].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[29].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[30].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_pll.spi_pll_recv[31].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.sclk_reg_dffrs
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.csn_reg_dffrs
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.mosi_reg_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.cnt_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.initaddr_vld_r_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.initaddr_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.cmd_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.chipid_vld_r_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.chipid_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.state_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.second_falling_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.addr_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.wrdata_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.wren_r_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.wren_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.rden_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.rddata_reg_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_dout_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.oen_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[0].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[1].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[2].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[3].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[4].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[5].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[6].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[7].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[8].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[9].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[10].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[11].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[12].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[13].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[14].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[15].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[16].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[17].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[18].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[19].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[20].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[21].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[22].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[23].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[24].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[25].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[26].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[27].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[28].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[29].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[30].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_slave.U_spi_sys.spi_sys_recv[31].spi_din_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[0].CMD_REG.rwaddr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[0].CMD_REG.wrdata_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[0].CMD_REG.wren_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[0].CMD_REG.reen_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[1].CMD_REG.rwaddr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[1].CMD_REG.wrdata_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[1].CMD_REG.wren_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[1].CMD_REG.reen_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[2].CMD_REG.rwaddr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[2].CMD_REG.wrdata_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[2].CMD_REG.wren_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[2].CMD_REG.reen_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[3].CMD_REG.rwaddr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[3].CMD_REG.wrdata_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[3].CMD_REG.wren_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_spi_bus_decoder.MAIN[3].CMD_REG.reen_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.testr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.sfrtr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.syncr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.syncr16_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.syncr16_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.sync_oen_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.rampctr_dfflrs
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.ramp_ifs_dfflrs
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.doselr_dfflrs
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdsftr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdstfr_dfflrs
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdstsr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdsthr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdstamr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdsdser_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdstaor_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.llvdssr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdsfcsr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdscecr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdsfstr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.lvdststr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.imr_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.cnt_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.sys_soft_rstn_r_dffls
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.rddata_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.train_ready_r_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.crc_error_r_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.cphase_adj_req_r_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.link_down_r_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.cmd_fifo_full_r_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.cmd_fifo_empty_r_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.isr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.misr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_systemregfile.irq_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_rst_gen_unit
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_rst_gen_unit.ch0_rstn_sync
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_rst_gen_unit.ch1_rstn_sync
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_rst_gen_unit.ch2_rstn_sync
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_rst_gen_unit.ch3_rstn_sync
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_SRC_INIT
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_SRC_INIT.SIM
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_SYNC_CLR_S
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_DEST_INIT
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_DEST_INIT.SIM
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_FB_DEST
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_FB_DEST.SIM
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_ACK
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_RST_SYNC.U_PS_ACK.SIM
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.u_dw_stream_sync.U_SYNC
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.U_prefill
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.U_prefill.delay_counter_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.U_prefill.prefill_start_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.U_prefill.prefilling_r_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.U_prefill.prefill_done_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.lane0_reg_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.lane1_reg_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.lane2_reg_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.lane3_reg_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.bit_counter_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.match_counter_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.state_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.delay_tap_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.tap_adj_req_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.link_down_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.train_ready_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.data_buf_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.match_head_start_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.data_counter_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.valid_int_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.descram_valid_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.data_in_reg_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_train.train_status_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_descrambler
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_descrambler.u0
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_descrambler.u1
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_descrambler.u2
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_descrambler.u3
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.u_fifo
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.u_fifo.spram
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.u_fifo.spram.bhv_spram
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.word_state_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.current_fifo_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.current_word_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.word_valid_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.data_len_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.data_cnt_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.state_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.cur_block_offset_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.block_done_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.base_addr_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.cur_block_addr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.cur_block_addr_r_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.wr_addr_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.wr_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.byte_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.wr_en_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.frame_done_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.u_crc32
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.crc_clear_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.crc_error_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.frame_status_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[0].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[1].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[2].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[3].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[4].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[5].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[6].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[7].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[8].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[9].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[10].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[11].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[12].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[13].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[14].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_block_data[15].cur_block_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[0].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[1].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[2].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[3].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[4].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[5].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[6].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[7].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[8].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[9].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[10].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[11].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[12].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[13].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[14].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dut.u_frame.gen_mask[15].cur_block_mask_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.sync_in_syncer
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.sync_in_syncer.data_temp0_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.sync_in_syncer.SYNCER[1].data_tempn0_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.sync_out_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.pulse_inst_sync
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.start_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.sync_start_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.state_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.cycle_num_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.base_addr_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.wave_leng_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.hold_leng_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.addr_cnt_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.wave_cnt_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.hold_cnt_c_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.sram_rd_en_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.sram_rd_addr_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.last_sram_rd_en_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.last_wave_data_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.last_rddata_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.wave_vld_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.hold_vld_n_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.hold_vld_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.wave_valid_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.awg_ctrl_inst.wave_data_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.cmd_fifo_inst
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.cmd_fifo_inst.spram
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.cmd_fifo_inst.spram.bhv_spram
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_sram_muxin
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_sram_muxout
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.U_sram_dmux_w
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U0_tsdn28hpcpuhdb4096x128m4mw_170a.MX
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U1_tsdn28hpcpuhdb4096x128m4mw_170a.MX
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U2_tsdn28hpcpuhdb4096x128m4mw_170a.MX
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[0].U3_tsdn28hpcpuhdb4096x128m4mw_170a.MX
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U0_tsdn28hpcpuhdb4096x128m4mw_170a.MX
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U1_tsdn28hpcpuhdb4096x128m4mw_170a.MX
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U2_tsdn28hpcpuhdb4096x128m4mw_170a.MX
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_awg_top.wave_dpram.U_tsmc_dpram.spram_512X8192_generation.genblk2[1].U3_tsdn28hpcpuhdb4096x128m4mw_170a.MX
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_ramp_gen
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.dacif_vld_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[0].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[1].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[2].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[3].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[4].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[5].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[6].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[7].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[8].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[9].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[10].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[11].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[12].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[13].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[14].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[15].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[16].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[17].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[18].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[19].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[20].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[21].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[22].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[23].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[24].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[25].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[26].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[27].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[28].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[29].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[30].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[31].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[32].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[33].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[34].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[35].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[36].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[37].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[38].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[39].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[40].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[41].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[42].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[43].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[44].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[45].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[46].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[47].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[48].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[49].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[50].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[51].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[52].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[53].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[54].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[55].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[56].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[57].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[58].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[59].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[60].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[61].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[62].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk1[63].mux_dfflr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[0].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[1].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[2].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[3].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[4].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[5].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[6].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[7].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[8].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[9].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[10].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[11].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[12].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[13].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[14].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[15].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[16].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[17].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[18].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[19].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[20].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[21].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[22].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[23].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[24].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[25].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[26].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[27].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[28].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[29].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[30].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[31].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[32].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[33].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[34].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[35].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[36].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[37].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[38].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[39].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[40].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[41].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[42].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[43].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[44].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[45].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[46].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[47].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[48].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[49].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[50].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[51].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[52].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[53].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[54].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[55].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[56].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[57].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[58].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[59].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[60].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[61].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[62].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.dacif_inst.genblk2[63].dout_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.rtermr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.prbsr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set0r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set1r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set2r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set3r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set4r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set5r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set6r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set7r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set8r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set9r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set10r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set11r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set12r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set13r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set14r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set15r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set16r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set17r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set18r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set19r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set20r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set21r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set22r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set23r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set24r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set25r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set26r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set27r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set28r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set29r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set30r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.set31r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.casaddrr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.casdwr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.imctr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.ibleedctr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.iclkcmlr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.currsvr0_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.currsvr1_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_dac_regfile.rddata_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalrstnr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.cclkdccenr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.casclkctr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccaldccqecpir_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalqecctr1_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.biasct3r_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalpictr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalcrossctr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalrsvr0_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ccalrsvr1_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.selck10gdr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.selck2p5gdr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.selck625mdr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.p2sdataenr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.enallpr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.enpipr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.clkdivrstnr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.p2srsvr0_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.p2srsvr1_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ckrxswr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.rstckr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.ctrzinr_dfflrd
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.U_clk_regfile.rddata_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.slv[0]
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.slv[1]
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.slv[2]
: Starting toggle coverage for module TB.U_da4008_chip_top.digital_top.slv[3]
: Starting toggle coverage for module TB.U_da4008_chip_top.DEM_VLD_dffr
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_0
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_1
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_2
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_3
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_4
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_5
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_6
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_7
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_8
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_9
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_10
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_11
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_12
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_13
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_14
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_15
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_16
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_17
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_18
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_19
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_20
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_21
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_22
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_23
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_24
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_25
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_26
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_27
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_28
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_29
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_30
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_31
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_32
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_33
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_34
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_35
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_36
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_37
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_38
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_39
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_40
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_41
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_42
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_43
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_44
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_45
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_46
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_47
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_48
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_49
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_50
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_51
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_52
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_53
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_54
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_55
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_56
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_57
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_58
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_59
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_60
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_61
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_62
: Starting toggle coverage for module TB.U_da4008_chip_top.U_DEM_PhaseSync_4008.inst_dem_64ch.inst_dem_63
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[0].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[1].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[2].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[3].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[4].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[5].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[6].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[7].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[8].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[9].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[10].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[11].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[12].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[13].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[14].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[15].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[16].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[17].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[18].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[19].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[20].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[21].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[22].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[23].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[24].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[25].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[26].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[27].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[28].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[29].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[30].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk1[31].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[32].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[33].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[34].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[35].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[36].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[37].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[38].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[39].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[40].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[41].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[42].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[43].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[44].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[45].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[46].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[47].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[48].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[49].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[50].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[51].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[52].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[53].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[54].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[55].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[56].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[57].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[58].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[59].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[60].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[61].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[62].U_DEM_Reverse
: Starting toggle coverage for module TB.U_DEM_Reverse_64CH.genblk2[63].U_DEM_Reverse
: Reporting line coverage at the end of simulation ...
: End of Line Coverage ...
: Reporting condition coverage at the end of simulation ...
: End of Condition Coverage ...
: Reporting branch coverage at the end of simulation ...
: End of Branch Coverage ...
: Coverage status: End of All Coverages ...

