sidCmdLineBehaviorAnalysisOpt -incr -clockSkew 0 -loopUnroll 0 -bboxEmptyModule 0  -cellModel 0 -bboxIgnoreProtected 0 
debImport "-sverilog" "-f" "filelist_vlg.f" "-top" "TB"
debLoadSimResult \
           /home/shbyang/Desktop/workplace/lin-win-share/DA4008_V1.2/sim/chip_top/work_RTL/sine_1g/verdplus_000.fsdb
wvCreateWindow
verdiWindowResize -win $_Verdi_1 "587" "176" "1057" "712"
srcHBSelect "TB.clk_40g_inst" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top.U_iopad" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top.digital_top" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top" -win $_nTrace1
srcSetScope -win $_nTrace1 "TB.U_da4008_chip_top" -delim "."
srcHBSelect "TB.U_da4008_chip_top" -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "MSB_OUT" -line 24 -pos 1 -win $_nTrace1
srcSelect -signal "LSB_OUT" -line 25 -pos 1 -win $_nTrace1
wvAddSignal -win $_nWave2 "/TB/U_da4008_chip_top/MSB_OUT\[63:0\]" \
           "/TB/U_da4008_chip_top/LSB_OUT\[63:0\]"
wvSetPosition -win $_nWave2 {("G1" 0)}
wvSetPosition -win $_nWave2 {("G1" 2)}
wvSetPosition -win $_nWave2 {("G1" 2)}
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
srcHBSelect "TB.U_da4008_chip_top.U_iopad" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top.digital_top" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top.digital_top" -win $_nTrace1
srcSetScope -win $_nTrace1 "TB.U_da4008_chip_top.digital_top" -delim "."
srcHBSelect "TB.U_da4008_chip_top.digital_top" -win $_nTrace1
srcSelect -signal "wave_data_valid" -line 53 -pos 1 -win $_nTrace1
srcSelect -signal "wave_data_out" -line 52 -pos 1 -win $_nTrace1
wvSetPosition -win $_nWave2 {("G1" 0)}
wvSetPosition -win $_nWave2 {("G1" 1)}
wvSetPosition -win $_nWave2 {("G1" 0)}
wvSetPosition -win $_nWave2 {("G2" 0)}
wvAddSignal -win $_nWave2 "/TB/U_da4008_chip_top/digital_top/wave_data_valid" \
           "/TB/U_da4008_chip_top/digital_top/wave_data_out\[63:0\]"
wvSetPosition -win $_nWave2 {("G2" 0)}
wvSetPosition -win $_nWave2 {("G2" 2)}
wvSetPosition -win $_nWave2 {("G2" 2)}
wvSetPosition -win $_nWave2 {("G2" 2)}
wvSetPosition -win $_nWave2 {("G2/digital_top" 0)}
wvAddSubGroup -win $_nWave2 -holdpost {digital_top}
wvAddSignal -win $_nWave2 "/TB/U_da4008_chip_top/digital_top/clk" \
           "/TB/U_da4008_chip_top/digital_top/rst_n" \
           "/TB/U_da4008_chip_top/digital_top/sync_in" \
           "/TB/U_da4008_chip_top/digital_top/sync_out" \
           "/TB/U_da4008_chip_top/digital_top/cfgid\[4:0\]" \
           "/TB/U_da4008_chip_top/digital_top/sclk" \
           "/TB/U_da4008_chip_top/digital_top/csn" \
           "/TB/U_da4008_chip_top/digital_top/mosi" \
           "/TB/U_da4008_chip_top/digital_top/miso" \
           "/TB/U_da4008_chip_top/digital_top/oen" \
           "/TB/U_da4008_chip_top/digital_top/irq" \
           "/TB/U_da4008_chip_top/digital_top/wave_data_out\[63:0\]" \
           "/TB/U_da4008_chip_top/digital_top/wave_data_valid" \
           "/TB/U_da4008_chip_top/digital_top/lvds_data\[3:0\]" \
           "/TB/U_da4008_chip_top/digital_top/lvds_valid\[0:0\]" \
           "/TB/U_da4008_chip_top/digital_top/lvds_clk\[0:0\]" \
           "/TB/U_da4008_chip_top/digital_top/phase_tap\[2:0\]" \
           "/TB/U_da4008_chip_top/digital_top/Rterm\[3:0\]" \
           "/TB/U_da4008_chip_top/digital_top/PrbsEn" \
           "/TB/U_da4008_chip_top/digital_top/Set\[63:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CasAddr\[2:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CasDw\[2:0\]" \
           "/TB/U_da4008_chip_top/digital_top/IMainCtrl\[9:0\]" \
           "/TB/U_da4008_chip_top/digital_top/IBleedCtrl\[3:0\]" \
           "/TB/U_da4008_chip_top/digital_top/ICkCml\[3:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CurRsv0\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CurRsv1\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CcalRstn\[0:0\]" \
           "/TB/U_da4008_chip_top/digital_top/EnAllP\[3:0\]" \
           "/TB/U_da4008_chip_top/digital_top/DccEn\[0:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CasGateCkCtrl\[0:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiEnPi\[0:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiEnQec\[0:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiEnDcc\[0:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiQecCtrlIp\[4:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiQecCtrlIn\[4:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiQecCtrlQp\[4:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiQecCtrlQn\[4:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiDccCtrlIup\[5:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiDccCtrlIdn\[5:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiDccCtrlQup\[5:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiDccCtrlQdn\[5:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiSiqNOut\[7:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiSiqPOut\[7:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiSiPOut\[3:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SpiSqPOut\[3:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CrtlCrossOverN\[2:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CrtlCrossOverP\[2:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CcalRsv0\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CcalRsv1\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SelCk10GDig\[3:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SelCk2p5GDig\[3:0\]" \
           "/TB/U_da4008_chip_top/digital_top/SelCk625MDig\[8:0\]" \
           "/TB/U_da4008_chip_top/digital_top/P2sDataEn\[15:0\]" \
           "/TB/U_da4008_chip_top/digital_top/P2sEnAllP\[15:0\]" \
           "/TB/U_da4008_chip_top/digital_top/EnPiP\[15:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CkDivRstn\[15:0\]" \
           "/TB/U_da4008_chip_top/digital_top/p2srsv0\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/p2srsv1\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CkRxSw\[15:0\]" \
           "/TB/U_da4008_chip_top/digital_top/RstnCk\[15:0\]" \
           "/TB/U_da4008_chip_top/digital_top/CtrlZin\[15:0\]"
wvSetPosition -win $_nWave2 {("G2/digital_top" 0)}
wvSetPosition -win $_nWave2 {("G2/digital_top" 62)}
wvSetPosition -win $_nWave2 {("G2" 2)}
wvSetPosition -win $_nWave2 {("G2" 2)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]" 0)}
wvAddSubGroup -win $_nWave2 -holdpost {slv[3:0]}
wvAddSubGroup -win $_nWave2 -holdpost {slv[3](sram_if)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]" 0)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[3](sram_if)" 0)}
wvAddSignal -win $_nWave2 "/TB/U_da4008_chip_top/digital_top/slv\[3\]/clk" \
           "/TB/U_da4008_chip_top/digital_top/slv\[3\]/addr\[19:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[3\]/din\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[3\]/dout\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[3\]/rden" \
           "/TB/U_da4008_chip_top/digital_top/slv\[3\]/wren" \
           "/TB/U_da4008_chip_top/digital_top/slv\[3\]/wben\[3:0\]"
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[3](sram_if)" 0)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[3](sram_if)" 7)}
wvSetPosition -win $_nWave2 {("G2" 2)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]" 0)}
wvAddSubGroup -win $_nWave2 -holdpost {slv[2](sram_if)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]" 0)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[2](sram_if)" 0)}
wvAddSignal -win $_nWave2 "/TB/U_da4008_chip_top/digital_top/slv\[2\]/clk" \
           "/TB/U_da4008_chip_top/digital_top/slv\[2\]/addr\[19:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[2\]/din\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[2\]/dout\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[2\]/rden" \
           "/TB/U_da4008_chip_top/digital_top/slv\[2\]/wren" \
           "/TB/U_da4008_chip_top/digital_top/slv\[2\]/wben\[3:0\]"
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[2](sram_if)" 0)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[2](sram_if)" 7)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]" 0)}
wvAddSubGroup -win $_nWave2 -holdpost {slv[1](sram_if)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]" 0)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[1](sram_if)" 0)}
wvAddSignal -win $_nWave2 "/TB/U_da4008_chip_top/digital_top/slv\[1\]/clk" \
           "/TB/U_da4008_chip_top/digital_top/slv\[1\]/addr\[19:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[1\]/din\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[1\]/dout\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[1\]/rden" \
           "/TB/U_da4008_chip_top/digital_top/slv\[1\]/wren" \
           "/TB/U_da4008_chip_top/digital_top/slv\[1\]/wben\[3:0\]"
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[1](sram_if)" 0)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[1](sram_if)" 7)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]" 0)}
wvAddSubGroup -win $_nWave2 -holdpost {slv[0](sram_if)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]" 0)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[0](sram_if)" 0)}
wvAddSignal -win $_nWave2 "/TB/U_da4008_chip_top/digital_top/slv\[0\]/clk" \
           "/TB/U_da4008_chip_top/digital_top/slv\[0\]/addr\[19:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[0\]/din\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[0\]/dout\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[0\]/rden" \
           "/TB/U_da4008_chip_top/digital_top/slv\[0\]/wren" \
           "/TB/U_da4008_chip_top/digital_top/slv\[0\]/wben\[3:0\]"
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[0](sram_if)" 0)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]/slv[0](sram_if)" 7)}
wvSetPosition -win $_nWave2 {("G2/slv[3:0]" 0)}
wvSetPosition -win $_nWave2 {("G2" 2)}
wvSetPosition -win $_nWave2 {("G2" 2)}
wvSetPosition -win $_nWave2 {("G2/mst(sram_if)" 0)}
wvAddSubGroup -win $_nWave2 -holdpost {mst(sram_if)}
wvAddSignal -win $_nWave2 "/TB/U_da4008_chip_top/digital_top/mst/clk" \
           "/TB/U_da4008_chip_top/digital_top/mst/addr\[24:0\]" \
           "/TB/U_da4008_chip_top/digital_top/mst/din\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/mst/dout\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/mst/rden" \
           "/TB/U_da4008_chip_top/digital_top/mst/wren" \
           "/TB/U_da4008_chip_top/digital_top/mst/wben\[3:0\]"
wvSetPosition -win $_nWave2 {("G2/mst(sram_if)" 0)}
wvSetPosition -win $_nWave2 {("G2/mst(sram_if)" 7)}
wvSetPosition -win $_nWave2 {("G2" 2)}
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollUp -win $_nWave2 34
wvSetPosition -win $_nWave2 {("G2" 0)}
wvCollapseGroup -win $_nWave2 "G2"
wvSelectGroup -win $_nWave2 {G2}
wvCut -win $_nWave2
wvSetPosition -win $_nWave2 {("G3" 0)}
wvSetPosition -win $_nWave2 {("G1" 2)}
wvSelectGroup -win $_nWave2 {G1}
wvCut -win $_nWave2
wvSetPosition -win $_nWave2 {("G3" 0)}
srcDeselectAll -win $_nTrace1
srcSelect -signal "wave_data_out" -line 52 -pos 1 -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "wave_data_valid" -line 53 -pos 1 -win $_nTrace1
srcHBSelect "TB.spi_bus" -win $_nTrace1
srcHBSelect "TB.clk_inst" -win $_nTrace1
srcHBSelect "TB.clk_40g_inst" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top" -win $_nTrace1
srcSetScope -win $_nTrace1 "TB.U_da4008_chip_top" -delim "."
srcHBSelect "TB.U_da4008_chip_top" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top.U_DEM_PhaseSync_4008" -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "LSB_OUT" -line 25 -pos 1 -win $_nTrace1
srcSelect -signal "MSB_OUT" -line 24 -pos 1 -win $_nTrace1
wvAddSignal -win $_nWave2 "/TB/U_da4008_chip_top/LSB_OUT\[63:0\]" \
           "/TB/U_da4008_chip_top/MSB_OUT\[63:0\]"
wvSetPosition -win $_nWave2 {("G3" 0)}
wvSetPosition -win $_nWave2 {("G3" 2)}
wvSetPosition -win $_nWave2 {("G3" 2)}
wvZoomOut -win $_nWave2
wvSelectSignal -win $_nWave2 {( "G3" 1 2 )} 
wvSetRadix -win $_nWave2 -format UDec
srcDeselectAll -win $_nTrace1
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvSelectSignal -win $_nWave2 {( "G3" 2 )} 
srcDeselectAll -win $_nTrace1
srcSearchString "wave sram" -win $_nTrace1 -prev -case
srcSearchString "wave sram" -win $_nTrace1 -prev -case
srcSearchString "wave sram" -win $_nTrace1 -next -case
srcSearchString "wave sram" -win $_nTrace1 -next -case
srcSearchString "wave sram" -win $_nTrace1 -next -case
srcSearchString "wave sram" -win $_nTrace1 -next -case
srcHBSelect "TB.U_da4008_chip_top" -win $_nTrace1
srcSetScope -win $_nTrace1 "TB.U_da4008_chip_top" -delim "."
srcHBSelect "TB.U_da4008_chip_top" -win $_nTrace1
srcSearchString "wave sram" -win $_nTrace1 -prev -case
srcSearchString "awg_top" -win $_nTrace1 -next -case
srcSearchString "awg_top" -win $_nTrace1 -prev -case
srcSearchString "awg_top" -win $_nTrace1 -next -case
srcSearchString "awg_top" -win $_nTrace1 -next -case
srcSearchString "awg_top" -win $_nTrace1 -next -case
srcSearchString "awg_top" -win $_nTrace1 -next -case
srcSearchString "awg" -win $_nTrace1 -next -case
srcSearchString "awg" -win $_nTrace1 -prev -case
srcSearchString "awg" -win $_nTrace1 -prev -case
srcDeselectAll -win $_nTrace1
srcSelect -signal "PI_mosi" -line 8 -pos 1 -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top.digital_top" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top.DEM_VLD_dffr" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top.U_DEM_PhaseSync_4008" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top.U_iopad" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top.digital_top" -win $_nTrace1
srcHBSelect "TB.U_da4008_chip_top.digital_top" -win $_nTrace1
srcSetScope -win $_nTrace1 "TB.U_da4008_chip_top.digital_top" -delim "."
srcHBSelect "TB.U_da4008_chip_top.digital_top" -win $_nTrace1
srcSearchString "awg_top" -win $_nTrace1 -next -case
srcSearchString "awg_top" -win $_nTrace1 -next -case
srcSearchString "awg_top" -win $_nTrace1 -prev -case
srcSelect -win $_nTrace1 -range {381 381 1 1 4 11}
srcSearchString "awg_top" -win $_nTrace1 -prev -case
srcSelect -win $_nTrace1 -range {388 388 3 4 3 1}
nsMsgSwitchTab -tab general
srcSearchString "awg_top" -win $_nTrace1 -prev -case
srcSelect -win $_nTrace1 -range {388 388 1 2 1 1}
srcSearchString "awg_top" -win $_nTrace1 -prev -case
srcSelect -win $_nTrace1 -range {381 381 1 1 4 11}
srcSearchString "awg_top" -win $_nTrace1 -prev -case
srcSelect -win $_nTrace1 -range {388 388 3 4 3 1}
srcSearchString "awg_top" -win $_nTrace1 -prev -case
srcSelect -win $_nTrace1 -range {388 388 1 2 1 1}
srcSearchString "awg_top" -win $_nTrace1 -prev -case
srcSelect -win $_nTrace1 -range {381 381 1 1 4 11}
srcSearchString "awg_top" -win $_nTrace1 -prev -case
srcSelect -win $_nTrace1 -range {388 388 3 4 3 1}
srcSearchString "awg_top" -win $_nTrace1 -prev -case
srcSelect -win $_nTrace1 -range {388 388 1 2 1 1}
srcSearchString "awg_top" -win $_nTrace1 -prev -case
srcSelect -win $_nTrace1 -range {381 381 1 1 4 11}
wvSelectGroup -win $_nWave2 {G3}
wvCut -win $_nWave2
wvSetPosition -win $_nWave2 {("G2" 0)}
wvSelectGroup -win $_nWave2 {G2}
wvSelectGroup -win $_nWave2 {G2}
srcDeselectAll -win $_nTrace1
srcSelect -signal "awg_busy" -line 411 -pos 1 -win $_nTrace1
srcSelect -win $_nTrace1 -range {389 411 7 8 2 5} -backward
srcDeselectAll -win $_nTrace1
srcSelect -signal "sync_pulse" -line 391 -pos 1 -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "clk" -line 389 -pos 2 -win $_nTrace1
srcSelect -signal "ch0_rstn_o" -line 390 -pos 1 -win $_nTrace1
srcSelect -signal "sync_pulse" -line 391 -pos 1 -win $_nTrace1
srcSelect -signal "wave_awrdata" -line 392 -pos 2 -win $_nTrace1
srcSelect -signal "wave_awren" -line 393 -pos 2 -win $_nTrace1
srcSelect -signal "wave_arwaddr" -line 394 -pos 2 -win $_nTrace1
srcSelect -signal "wave_awrmask" -line 395 -pos 2 -win $_nTrace1
srcSelect -win $_nTrace1 -signal "slv\[2\].din" -line 396 -pos 1
srcSelect -win $_nTrace1 -signal "slv\[2\].wren" -line 397 -pos 1
srcSelect -win $_nTrace1 -signal "slv\[2\].addr\[18:0\]" -line 398 -pos 1
srcSelect -win $_nTrace1 -signal "slv\[2\].rden" -line 399 -pos 1
srcSelect -win $_nTrace1 -signal "slv\[2\].dout" -line 400 -pos 1
srcSelect -win $_nTrace1 -signal "slv\[1\].din" -line 401 -pos 1
srcSelect -win $_nTrace1 -signal "slv\[1\].wren" -line 402 -pos 1
srcSelect -win $_nTrace1 -signal "slv\[1\].wren" -line 402 -pos 1
srcSelect -win $_nTrace1 -signal "slv\[1\].addr\[7 :0\]" -line 403 -pos 1
srcSelect -win $_nTrace1 -signal "slv\[1\].wren" -line 402 -pos 1
srcSelect -win $_nTrace1 -signal "slv\[1\].rden" -line 404 -pos 1
srcSelect -win $_nTrace1 -signal "slv\[1\].dout" -line 405 -pos 1
srcSelect -signal "wave_data_out_bank" -line 406 -pos 1 -win $_nTrace1
srcSelect -signal "awg_data_valid" -line 407 -pos 1 -win $_nTrace1
srcSelect -signal "cmd_fifo_empty" -line 408 -pos 2 -win $_nTrace1
srcSelect -signal "cmd_fifo_full" -line 409 -pos 2 -win $_nTrace1
srcSelect -signal "awg_status" -line 410 -pos 1 -win $_nTrace1
srcSelect -signal "awg_busy" -line 411 -pos 1 -win $_nTrace1
wvAddSignal -win $_nWave2 "/TB/U_da4008_chip_top/digital_top/clk" \
           "/TB/U_da4008_chip_top/digital_top/ch0_rstn_o" \
           "/TB/U_da4008_chip_top/digital_top/sync_pulse" \
           "/TB/U_da4008_chip_top/digital_top/wave_awrdata\[511:0\]" \
           "/TB/U_da4008_chip_top/digital_top/wave_awren\[0:0\]" \
           "/TB/U_da4008_chip_top/digital_top/wave_arwaddr\[12:0\]" \
           "/TB/U_da4008_chip_top/digital_top/wave_awrmask\[63:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[2\]/din\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[2\]/wren" \
           "/TB/U_da4008_chip_top/digital_top/slv\[2\]/addr\[18:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[2\]/rden" \
           "/TB/U_da4008_chip_top/digital_top/slv\[2\]/dout\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[1\]/din\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[1\]/addr\[7:0\]" \
           "/TB/U_da4008_chip_top/digital_top/slv\[1\]/wren" \
           "/TB/U_da4008_chip_top/digital_top/slv\[1\]/rden" \
           "/TB/U_da4008_chip_top/digital_top/slv\[1\]/dout\[31:0\]" \
           "/TB/U_da4008_chip_top/digital_top/wave_data_out_bank\[511:0\]" \
           "/TB/U_da4008_chip_top/digital_top/awg_data_valid" \
           "/TB/U_da4008_chip_top/digital_top/cmd_fifo_empty" \
           "/TB/U_da4008_chip_top/digital_top/cmd_fifo_full" \
           "/TB/U_da4008_chip_top/digital_top/awg_status\[2:0\]" \
           "/TB/U_da4008_chip_top/digital_top/awg_busy"
wvSetPosition -win $_nWave2 {("G2" 0)}
wvSetPosition -win $_nWave2 {("G2" 23)}
wvSetPosition -win $_nWave2 {("G2" 23)}
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollDown -win $_nWave2 0
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 0
wvScrollDown -win $_nWave2 0
wvScrollDown -win $_nWave2 0
wvScrollDown -win $_nWave2 0
wvScrollDown -win $_nWave2 0
wvScrollDown -win $_nWave2 0
wvSetCursor -win $_nWave2 135609782.382826 -snap {("G2" 22)}
wvSelectSignal -win $_nWave2 {( "G2" 21 )} 
wvSelectSignal -win $_nWave2 {( "G2" 22 )} 
wvSelectSignal -win $_nWave2 {( "G2" 20 )} 
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvZoomIn -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvSelectSignal -win $_nWave2 {( "G2" 8 )} 
wvSelectSignal -win $_nWave2 {( "G2" 7 )} 
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollUp -win $_nWave2 1
wvScrollDown -win $_nWave2 0
wvScrollDown -win $_nWave2 0
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvScrollDown -win $_nWave2 1
wvSelectSignal -win $_nWave2 {( "G2" 12 )} 
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomIn -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
debExit
