sidCmdLineBehaviorAnalysisOpt -incr -clockSkew 0 -loopUnroll 0 -bboxEmptyModule 0  -cellModel 0 -bboxIgnoreProtected 0 
debImport "-sverilog" "-f" "filelist_vlg.f" "-top" "TB"
debLoadSimResult \
           /home/shbyang/Desktop/workplace/therm_design/sim/therm_chip_top/wave.fsdb
wvCreateWindow
verdiWindowResize -win $_Verdi_1 "239" "111" "1440" "723"
srcHBSelect "TB.u_digital_top" -win $_nTrace1
srcHBSelect "TB.Unnamed_\$TB_sv_88" -win $_nTrace1
srcHBSelect "TB.Unnamed_\$TB_sv_88" -win $_nTrace1
srcSetScope -win $_nTrace1 "TB.Unnamed_\$TB_sv_88" -delim "."
srcHBSelect "TB.Unnamed_\$TB_sv_88" -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcHBSelect "TB.gen_pulses" -win $_nTrace1
srcHBSelect "TB.send_byte" -win $_nTrace1
srcHBSelect "TB.u_digital_top" -win $_nTrace1
srcHBSelect "TB.u_digital_top" -win $_nTrace1
srcHBSelect "TB.u_digital_top" -win $_nTrace1
srcSetScope -win $_nTrace1 "TB.u_digital_top" -delim "."
srcHBSelect "TB.u_digital_top" -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "temp_85_fre_k" -line 74 -pos 2 -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "temp_neg_40_fre_k" -line 75 -pos 2 -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "temp_85_fre_k" -line 74 -pos 2 -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "temp_neg_40_fre_k" -line 89 -pos 2 -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "report_en" -line 90 -pos 2 -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "temp_neg_40_fre_k" -line 89 -pos 2 -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "out_mode" -line 87 -pos 2 -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "rep_gap_us" -line 91 -pos 2 -win $_nTrace1
srcAddSelectedToWave -clipboard -win $_nTrace1
wvDrop -win $_nWave2
srcDeselectAll -win $_nTrace1
srcSelect -signal "therm_out" -line 92 -pos 2 -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "therm_out" -line 92 -pos 2 -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcDeselectAll -win $_nTrace1
srcSelect -signal "therm_out" -line 92 -pos 2 -win $_nTrace1
srcAddSelectedToWave -clipboard -win $_nTrace1
wvDrop -win $_nWave2
srcDeselectAll -win $_nTrace1
srcSelect -signal "therm_vld" -line 93 -pos 2 -win $_nTrace1
srcAddSelectedToWave -clipboard -win $_nTrace1
wvDrop -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
wvZoomOut -win $_nWave2
srcHBSelect "TB.u_digital_top.u_digital_thermometer" -win $_nTrace1
srcHBSelect "TB" -win $_nTrace1
srcSetScope -win $_nTrace1 "TB" -delim "."
srcHBSelect "TB" -win $_nTrace1
srcDeselectAll -win $_nTrace1
verdiWindowResize -win $_Verdi_1 "270" "72" "1440" "723"
